TAPI-Environment • Speed Dial Buttons / Monitor Bar • Least Cost Routing (LCR) / Charge • TAPI Monitor
Integrated TAPI drivers • TAPI devices and drivers • Network TAPI
<< Up >> | ### TAPI devices and drivers | Page Index
Tested TAPI Devices

TAPI device | TAPI Configuration / TAPI Driver
Siemens Gigaset product family | Hints for TAPI configuration of the Gigaset SX353isdn: Start your Siemens Talk&Surf application. Choose [Configuration > System Settings] Under [Device Assigment] the option [Link Phone with PC] is to be activated. Choose an internal line from the list. Run the xtelsio CTI Client. Under [Options > TAPI Devices > Add > Local TAPI Devices] select "Line 0 on HUB Device". Recognition of incoming phone calls: Unfortunately, the driver TAPI do not announces phone numbers for incoming phone calls. If you have an ISDN card in your computer, you can use the option "Use ISDN card call monitor". Incoming phone calls are recognised via CAPI interface then. You find the option under: [Options > TAPI Devices...] Other pages for Siemens Gigaset SX353isdn: Very extensive side with tips and tricks to Siemens Gigaset product family: http://sg.xinfo.net/#TAPI
Ascotel Office 30 | Entrance side to the download the TAPI driver Direct download link
Europe 30i | Download TAPI Driver