Versions • Installation • Program Features • Folders / Data Linking • Telephone Control • Options
TAPI-Environment • Speed Dial Buttons / Monitor Bar • Least Cost Routing (LCR) / Charge • TAPI Monitor
Up >> | ### TAPI-Environment | Page Index
Integrated TAPI drivers • TAPI devices and drivers • Network TAPI

The phone control of xtelsio CTI Client is based on Windows TAPI interface. So you can control and monitor all phones for which a TAPI driver is installed on your computer.
| TAPI Enviroments
| PBX, Workplace-CTI If you want to use CTI only for one workplace on an small PBX, install on this computer the TAPI driver of the PBX and configure one of the lines offered by the TAPI driver in the CTI Client application.
| Network If you want to use the application on several network clients whose phones can be controled only by the TAPI driver of the PBX, then you need: the xtelsio CTI Server or a TAPI Server. xtelsio CTI Server provides the TAPI devices of the server to several xtelsio CTI Clients on the network. The xtelsio CTI Clients have a special Server-Connector. Other TAPI applications cannot be used via xtelsio CTI Server. More infos... TAPI Server offers the TAPI devices of the server via TAPI interface. Cn the client, any TAPI applications can be used therefore. More infos...
| ISDN Phone with V.24 / USB Install the TAPI driver of the phone on your computer and then configure this TAPI device in the CTI Client. Analogous phone with V.24 This variant works, for example, with tiptel 175 clip which provides an own TAPI driver.
| Analogous Phone + Modem In the simplest case you can use for analogous phones the TAPI modem driver to dial phone numbers.
| Integrated CAPI driver
| ISDN Card + Headset The integrated CAPI driver connects the ISDN card and sound card of your computer and allows thus the phoning via Headset. Warning: Besides, by system short speech delays appear and it can result in echo effects. Tested with AVM Fritz-Card.