Integrated TAPI drivers • TAPI devices and drivers • Network TAPI
Up | ### Tested TAPI Devices | Page Index

Problems with TAPI devices?
With xtelsio CTI Client you can manage and monitor all phones and PBX' for which a TAPI driver is provided. Because the TAPI serve as a general-valid interface for a huge number of existing and future telephony hardware, their specification is variable in some points. In what can the behaviour of the TAPI drivers vary? Support of optional functions such as: Consultation, Hold, Toggle, Conference, Transfer, Call Forwarding, Display Messages, ... Call State Events: The TAPI drivers send with call setup, with incoming phone call, with consultation and other relevant actions state event messages to the TAPI application. The type and the order of the state events can vary according to TAPI driver or also in dependence of the software version of the PBX. If the application has problems with the state events of your TAPI driver, you can log these events with the TAPI monitor. You can activate{energise} the TAPI monitor about [Menu> options> TAPI monitor]. For an adaptation of the CTI Client to your TAPI driver, please send the monitor output with a small note to info@xtelsio.de.
xtelsio CTI Client was tested with following devices:
Siemens Telas Server 3.1 HiPath 4000 + CAP Server OptiPoint 500 USB + HiPath 4000
TELEBAU Elektro- und Fernmeldetechnik GmbH ISDN PBX TELNET TKS ISDN PBX TELNET Daniel ISDN system phone JULIA ISDN comfort phone NINA
elmeg ISDN PBX elmeg C44 ISDN PBX elmeg C46xe
Alcatel OmniPCX Office, Soft Release R3
With the following devices (and others) the application is in use:
Philips ErgoLine D330/D340 Eumex 404 europa30i elmeg C3x0 elmeg C64 Gigaset SX323 Auerswald COMpact 4410 Auerswald COMfort 2000 phone Ericsson MD110 Line t-comfort 730 tiptel 175 clip OptiSet at Hicom 150 E AGFEO AS40P Cisco IP PBX Panasonic KX-TD octopus open Fritz AVM Card DeTeWe OpenCom 100 Asterisk PBX