TAPI-Environment • Speed Dial Buttons / Monitor Bar • Least Cost Routing (LCR) / Charge • TAPI Monitor
Speed Dial Button - Settings • Phone Status LEDs
Up >> | ### Speed Dial Button - Settings | Page Index

In this dialog you can set properties for a speed dial button. Action Type Dial Phone Number: This is the default type. With a click to the speed dial button the phone number entered in phone number field is dialed. Dial Programming Code: This action type can be used to dial specific programming codes. Example:switch-on/off the night service of your PBX Open File: To open a file or folder. Open URL: With click to the speed dial button the web-page specified in URL is opened in your standard-browser. Start Program: A speed dial button click runs the specified file (EXE). Use the right button to select the EXE file. Use predefined action This option is only visible if there are predefined actions, for example if you have installed xtelsio CTI Client from a Driver-CD of a PBX and the manufacturer wants to provide specific predefined actions in connection with this PBX-. Name: = Name of the speed dial button Icon Here you can select optionally an icon or a small bitmap for the button. Icons should have the format 16x16 pixels. Global Hotkey You can assign a global hotkey to a speed dial button (for example the F11). Now you can hit the speed dial button by F11, also if the CTI Client is minimized. xtelsio must be running, however. If you assign a hotkey to a speed dial button of the monitor-bar, the monitor-bar must be activated to use the hotkey. TAPI Device/MSN If you have configured several TAPI devices or several MSNs to a TAPI device, you can assign it to a speed dial button. This can make sense, for instance if you use one MSN for business calls and another MSN for private calls.