Integrated TAPI drivers • TAPI devices and drivers • Network TAPI
xtelsio CTI Server • Asterisk • ISDN Card and Headset • Skype Connector • Idefisk BIZ • snom phones
<< Up >> | ### Idefisk BIZ | Page Index

xtelsio CTI client in use with Idefisk BIZ
Idefisk is an IAX-Softphone for Asterisk. The xtelsio CTI client contains a Connector for the business version of Idefisk. So you can setup, accept and hang up phone calls with xtelsio CTI client.
Integrate Idefisk in the CTI client
Select under [Options > TAPI devices> Add> VoIP] the "IdefiskBIZ Lines". In the current version there is still no driver-configuration dialog. All necessary settings have to be carried out directly in Idefisk.
Idefisk configuration in combination with xtelsio CTI client
If you run Idefisk before xtelsio CTI client, the following options have to be deactivated: [General Options > Automatic popup on incoming calls] [General Options > Popup menu on incomming calls]
Hints
If you start xtelsio CTI Client before Idefisk, Idefisk starts automatically in the background. Then the surface remains invisible, even if you run Idefisk afterwards by hand. While finishing xtelsio CTI Client the Idefisk instance is still running. The Idefisk process can be finished by the tast manager when required.