Versions • Installation • Program Features • Folders / Data Linking • Telephone Control • Options
Customize • Audio • TAPI Devices • Telephony • Journal • License • LCR/Charge • Interworking • History • Outlook • Word Document Templates • Terminal Server • Notes
<< Up >> | ### TAPI Devices | Page Index
Dial Settings

Configuration Dialog: [Options > TAPI Devices]
Local Profile
These settings are stored in a local profile directory. The local profile uses your computer name.
Control / Monitor these Devices
Add here all TAPI devices, witch you want to control / to observe. You can use the up/down button to set the TAPI device order in the main window.
Device properties
Show "Please pickup the receiver"-dialog: A corresponding dialog is shown before the dial-command is sent to the device. As soon as you pick up the receiver the dialog is automatically closed and the phone number is dialed. This option should be used for TAPI devices without automatic offhook. Call signaling by sound card: If you phone via sound-card (e.g. in combination with an ISDN card), you should activate this option. Modem: Set this option for analogue-modems. Use ISDN-Card for call monitor: With this setting incoming phone-calls are recognized by the ISDN-card and indicated in the CTI Client. This is a special Option for TAPI drivers supporting only outgoing calls. Buttons: Dial Settigns: Configuration of city/area code, phone number format and some more. Driver configuration: The driver configuration dialog is shown. Numbers: Select the phone numbers you want to control/monitor. This number is displayed below the receiver button in main view. Hint: The button is disabled if the TAPI driver supports only one number.