Dial Settings
Location • PBX • Format of Phone Numbers • Dial • Consultation / Hold • Error Handling
<< Up >> | ### PBX | Page Index

Configuration Dialog: [Options > TAPI Devices > Dial Settings > PBX] The settings refer to the shown PBX. Outside line access codes: Enter here the outside line access code(s) of your PBX. If you use '0' for business calls an '8' for private calls you have to enter '0,8'. Use the button "out" right to the receiver to switch between your outside line access codes. maximum length of internal numers: By this setting xtelsio distinguishs between internal and external numbers.