Data Sources • Tree Structure • Search • Sorting • New... • Importing Data • Filter • Cache, Refresh • Data Form • Properties
Name and Content • Data source • Column Selection • Column Properties • View • Cache • Properties
<< Up | ### Properties | Page Index
Birthday Warning

Write Protected: The content of the folder becomes write-protected. The user receives later an error message if he attempts to change, to modify or to delete a record. Hint: This flag is always set, when a text file was integrated from outside of the working directory. Reason: It is expected that the text file was exported from another application and the dates keep on being maintained in the other application. If the content of the text file was changed also in xtelsio CTI Client, a conflict would occurs with the next export from the other application. Protect Data Form: The data form is blocked against modifications, that is, the user can not move the fields anymore or change their properties. If you check "do not announce any birthdays from this folder" you will receive no birthday warnings. Otherwise you will receive 10 days before birthday becomes due a memory as an appointment. You can relocate the first notice for a week and so on. Limit call connected time: This is a special feature with which you can determine that you get a signal after a certain conversation time that the conversation should be ended slowly. If "Use as default import folder" is checked, data transfers of klickInvers (for example) are always added to this folder. If no folder has set this flag then Client application asks into which folder the record is supposed to be imported. PSTN digit (outside line access code): This setting is interesting only for PBX systems with several outside line access codes. So for example the 0 for business conversations and the 8 for private calls can be dialled. A folder that contains business contacts should use the outside line access code '0'. So you do not have to select the PSTN digit before every dialing. Here you can enter the list of all available PSTN digits. TAPI Device: You can use this option if you have configured several TAPI devices or a TAPI device that offers several MSNs. Here you can define folder specific which MSN is supposed to be used for outgoing phone calls. If no TAPI device is selected, the currently selected TAPI device/MSN is used. Notes field: If the primary data source contains a memo field, then you can determine here that the field contents should be shown in the notes window (and can be edited there). The memos are stored in the primary database and thus all users see the same memos.