Dial Settings
Location • PBX • Format of Phone Numbers • Dial • Consultation / Hold • Error Handling
<< Up >> | ### Dial | Page Index

Configuration Dialog: [Options > TAPI Devices > Dial Settings > Dial] By this option you can adjust some TAPI actions to work with the TAPI driver. Connection Type: Here you can define the parameter "MediaMode" for the TAPI-LineMakeCall-function. Default setting is "Voice connection". Change this parameter only if the TAPI-monitor reports an "INVALID_MEDIAMODE" after MakeCall. The originator's phone should be automatically taken offhook: If this option is set, the TAPI device is assigned explicitly to activate offhook-mode if you dial a phone number with hung up receiver. This TAPI parameter is not analyzed by all TAPI drivers. It can be therefore that the phone switches into the offhook-mode although this option is deactivated or turned around. Default setting: "activated" Suppress phone number transmission (CLIR): With this option the TAPI driver can be informed, that the own phone number is not supposed to be indicated at the destination station. Please test the option with a phone-call onto the own mobile-phone, to ensure that the TAPI driver masters this mode. Show "Please pickup the receiver"-dialog: This option should always be activated, if the TAPI driver can't activate the offhook-mode; e.g. with analogue phones or if you use the TAPI driver of a PBX-system. With the option "Show dialog first and then send dial-command.", the dialog waits for offhook and then dials the phone number with TAPI-function lineDial. It can be that this mode is not supported by your PBX. With the option "Send dial command first and then show dialog.", the application sends the TAPI-command lineMakeCall immediately to the telephone or PBX and then shows the dialog.