Standard Installation • Network Installation • Shared Address Data • Create Setup
Simple network-setup • Extended network-setup • Webserver-setup • Select Folders • Transfer Settings
<< Up | ### Transfer Settings | Page Index

Select in this dialog the settings which you want to take over into the preconfigured installation. License Key: The license key is entered into the file "cfg\licence.ini". TAPI Device(s): The transfer of the TAPI device configuration to another computer may be successful according to TAPI driver. LCR Table: Only available for Germany. Content of Speed Dial Buttons: You don't need this option normally since the users will define their own speed-dial-button on the cloned computer. Configuring an empty working directory later automatically: This is a special function for network environments. The administrator can automate the configuration of the individual computers. He have to provide only a program link with an empty working directory for the users. During the first start of the application the working directory will be configured automatically. The configuration is taken over from the sub-folder [auto_config\workingDir] of the program directory.