Versions • Installation • Program Features • Folders / Data Linking • Telephone Control • Options
Standard Installation • Network Installation • Shared Address Data • Create Setup
Up >> | ### Standard Installation | Page Index
Working Directory

Standard Installation
Steps: Un-zip the ZIP archive and then run setup.exe. Follow the dialog sequence. Hints: The setup creates only the most necessary Registry entries for the deinstallation as well as for the components ActiveX and TAPI-Connector. The Registry entries are not necessary for most installations. In this case you could install the software also by hand. The configuration data are stored not in the Registry, but in the Working Directory.
Installation by Hand
In some cases an installation by hand can be advantageous. The following steps are to be carried out: Un-zip the setup ZIP archive. For the installation you need only two folders: bin: This folder contains the program directory. workingDir: This folder contains the working directory. Copy the folder "bin" to " C:\Programme\" and rename this afterwards to "xtelsio_CTI_Client". Copy the folder "workingDir" to "My Files" and rename it afterwards to "xtelsio_CTI_Client_Data". Create a program shortcut on the desktop: Drag the xtelsio.exe from "C:\Programme\xtelsio_CTI_Client" with the right mouse key on the desktop and choose in the appearing context menu the entry [Create Shortcuts Here]. Right-click the new program shortcut and enter under "Start in:" the path to your working directory (see 3.). That's all.