TAPI for snom
Installation • Configuration Pages:
Up >> | ### Installation | Page Index

How to set-up xtelsio TAPI for snom:
1. Download and Installation
Download und extract xtelsio_TAPI_for_snom_setup.zip. Run setup.exe and follow the dialogs.
2. TAPI Driver Configuration
You can open the driver configuration via: [Start > Programs > xtelsio_TAPI_for_snom > xtelsio TAPI for snom - Configuration > Configure...].
Hint: At first, only one TAPI line is supported Double-clicking the TAPI line opens the dialog shown right. |
Futher hints for configuration see: Connection Actions URL
If these settings are done the TAPI driver should work now.
4. Test with Outlook
Close and restart Outlook Right click one of your Outlook contacts and select "Call Contact...". Click to dialog button "Dialling Options..." Select your "Asterisk Line" in the pull down list in section "Connect using line". Hint: You may need to scroll in the pull down list to see all TAPI Lines. Close this dialog with [OK]. Now you are able to make calls via Outlook.
5. Test with xtelsio CTI Client lite
"xtelsio CTI Client lite" is a freeware TAPI application. Download and extract xtelsio_CTI_Client_lite_setup.zip. Run setup.exe and follow the dialogs. Start xtelsio CTI Client. Select [Options > TAPI-Devices > Add] You should see your Asterisk Lines in the appearing dialog window. A double-click to one line closes the dialog and adds the line to the device list. Close this dialog with [OK]. A Location config dialog may appear, if location parameters are unknown. Now you can enter a phone number right to the dial button and dial it by pressing the enter key or by mouse click.