Connection • Dial • Actions URL
Up | ### Firewall Configuration | Page Index

If you use a firewall on your PC you may need to enable the micro webserver TCP port manually for incoming HTTP connections from snom phone. If the filrewall blocks incomming TCP connections, you don't get any TAPI call events. Example configuration for Windows XP Firewall for TCP port 88: Open the firewall configuration by: [Start > Control Panel > Security Center > Windows Firewall] Select Page "Exceptions" Click to button [Port...] Enter a name, for instance: "enable TCP port 88 for snom TAPI" Enter port number "88" an click [OK].