Connection • Properties
Asterisk Manager • Asterisk Manager Proxy
<< Up | ### Asterisk Manager Proxy | Page Index

Asterisk Manager Proxy
The Asterisk Manager Proxy should be used if more then 10 Clients needs a connection to Manager or if you need additional security functions. More infos for the Asterisk Manager Proxy are available at: http://www.voip-info.org/wiki/view/AstManProxy Configuration Files: The Asterisk Manager Proxy configuration files are "astmanproxy.conf" and "astmanproxy.users".
astmanproxy.conf
The following parameters of astmanproxy.conf are of interest for the TAPI driver:
; astmanproxy.conf ... acceptunencryptedconnection = yes listenaddress = * listenport = 1234 authrequired = yes/no proxykey = secret inputformat = standard outputformat = standard
Comments: |
acceptunencryptedconnection | must be "yes"
listenaddress listenport | The TAPI driver connects to this IP address and port.
authrequired | "yes" or "no"
proxykey | If set, the "secret" must also be set in the Asterisk Server Dialog.
inputformat outputformat | must be "standard"
astmanproxy.users
; Astmanproxy user list ; ; Reload permissions by sending a SIGHUP ; ; "user" is the username, secret is the password, and the (optional) ; channel setting causes filtering of events only for the specified ; channel to be sent to this user. ; ; user=secret,channel,out_context (to Asterisk),in_context (From Asterisk) steve=steve,SIP/snom190,local,
Comment: If you set a channel like "SIP/snom190" for a user some call states can't be detected, for example "RINGBACK".