Installation • Asterisk Server Configuration • Special Devices
Connection • Properties
Up >> | ### Connection | Page Index
Asterisk Manager • Asterisk Manager Proxy

Configuration Dialog: [TAPI-Line Configuration> Asterisk Server> Settings... > Connection]
Asterisk Manager access
The TAPI driver uses the functions of the Asterisk Manager via TCP/IP connection. There are two ways to access the Asterisk Manager: the direct access to the Asterisk Manager or via Asterisk Manager Proxy
"Asterisk Server" Dialog
In dialog "Asterisk Server" you have to enter the access parameters for the Asterisk Manager Interface or the Asterisk Manager Proxy. The right dialog image shows a successful Connect and Login. IP-Address: IP address or host name of server running the Asterisk Manager Port: Must be equal to parameter "port" in manager.conf! Username: the user you set-up in "manager.conf" Password: the users secret you set-up in "manager.conf"
Example for Asterisk Manager Proxy: |