Connection • Properties
Asterisk Manager • Asterisk Manager Proxy
Up >> | ### Asterisk Manager | Page Index
manager_custom.conf

Asterisk Manager account setup
You need an account to access the Asterisk Manager Interface. The accounts are stored in the Asterisk configuration file "manager.conf" or "manager_custom.conf". Example of manager.conf:
; ; Asterisk Call Management support ; [general] enabled = yes port = 5038 bindaddr = 0.0.0.0 [admin] secret= amp111 deny=0.0.0.0/0.0.0.0 permit=127.0.0.1/255.255.255.0 read = system,call,log,verbose,command,agent,user write = system,call,log,verbose,command,agent,user [AstTapi] secret= AstTapi deny=0.0.0.0/0.0.0.0 permit=192.168.0.0/255.255.255.0 read = system,call,log,verbose,command,agent,user write = system,call,log,verbose,command,agent,user #include manager_custom.conf
Comments: |
[AstTapi] | The section [AstTapi] was added to manager.conf. "AstTapi" is the login name you can use later.
secret= AstTapi | = Password
permit= 192.168.0.0/255.255.255.0 | All computers with an IP address in range 192.168.0.xxx can use this account.
#include manager_custom.conf | Alternatively you can add the account also to manager_custom.conf.Beispiel
Hint: Please reload the Asterisk Manager to activate the new or modified account!