Installation • Asterisk Server Configuration • Special Devices
Connection • Properties
<< Up | ### Properties | Page Index
Extended TAPI Functions - Description

Configuration Dialog: [TAPI-Line Configuration > Asterisk Server > Settings... > TAPI-Functions]
Support Extended TAPI Functions
Available extended TAPI functions: Consultation / Transfer Conference Hold These functions need the context [tapi-conference-control] for dynamic conference management in <extension.conf>.
[tapi-conference-control] exten => 9000,1,MeetMe(|M1deq) exten => _X,1,MeetMe(${EXTEN}|1) exten => _XX,1,MeetMe(${EXTEN}|1) exten => _XXX,1,MeetMe(${EXTEN}|1)
Comments: |
[tapi-conference-control] | If you rename this context you have to change it in the configuration dialog too.
9000 | This is a virtual phone number to create a dynamic conference room. If you chage this number you have to change it in the configuration dialog too.
_X, _XX, _XXX | The entries are needed to add calls into a conference.
Example extract from extensions.conf:
... ; ###################################################################### ; Extension Contexts [ext] ; ###################################################################### [tapi-conference-control] exten => 9000,1,MeetMe(|M1deq) exten => _X,1,MeetMe(${EXTEN}|1) exten => _XX,1,MeetMe(${EXTEN}|1) exten => _XXX,1,MeetMe(${EXTEN}|1) [ext-zapbarge] exten => 888,1,SetGroup(${CALLERIDNUM}) exten => 888,2,Answer exten => 888,3,Wait(1) exten => 888,4,ZapBarge exten => 888,5,Hangup [ext-meetme] exten => _8X,1,Answer exten => _8X,2,Wait(1) exten => _8X,3,GotoIf($[${CALLERIDNUM} = ${EXTEN:1}]?5:4) exten => _8X,4,MeetMe(${EXTEN}|sM) exten => _8X,5,MeetMe(${EXTEN}|asM) ...
Hint: Please reload the Asterisk Manager to activate the modified settings!