Installation • Configuration Pages:
Connection • Dial • Actions URL
<< Up >> | ### Dial | Page Index

Identity for Outgoing Calls
If you have entered multiple identities in your snom phone you can select one for outgoing calls: via snom configuration or via TAPI application (temporary)
Re-scan identities from snom phone. | Set this check box if you have changed the identities configuration of your snom phone and you want to select the identity via TAPI application. The TAPI driver scans the identities with next TAPI application start (lineGetDevCaps).
TAPI Functions
Consultation | Set this check box if you want to initiate consultation calls with your TAPI application. Be aware what ony consultation is supported via TAPI, but no reconnect or transfer. You have to use the keys of your snom phone for these functions.
Detect Special States
"Hang Up" after redirect incoming call | The log file is analysed to detect the hangup state of your snom phone after you have redirected an incoming call.